--------------------------------------------------------------------------------
FtMscLib.dll Version  01.05.11  (2012/02/19)
FtLogLevel= 0
23:01:58:593, Initialization of Library 'ftMscLib.dll' ...

INFO:   size FTX1_SHMIFINFO   = 64
INFO:   size FTX1_STATE       = 100
INFO:   size FTX1_CONFIG      = 88
INFO:   size FTX1_INPUT       = 68
INFO:   size FTX1_OUTPUT      = 44
INFO:   size FTX1_DISPLAY     = 108
INFO:   size TRANSFER_STATUS  = 4
INFO:   size CHANGE_STATE     = 8
INFO:   size RP_TIMER         = 12
INFO:   size MOTOR            = 24
INFO:   size INPUT_SIM        = 4
INFO:   size HOOK_TABLE       = 140
INFO:   RESERVE_SIZE          = 360
INFO:   size FISH_X1_TRANSFER = 1024
INFO: size IF08_MAX           = 9
INFO: size IF08_TRANSFER      = 9216

23:01:58:593, Creating event objects...
23:01:58:593, Starting thread [WaitMmRpTmEvent]...
23:01:58:593,   [WaitMmRpTmEvent] started, hRpTmThrWait= 520
23:01:58:593, Starting thread [WaitMmEvent]...
23:01:58:593,   [WaitMmEventThread] started, hThrWait= 528
23:01:58:593, Starting thread [FtRequestThread]...
23:01:58:593,   [FtRequestThread] started, hThrRequest= 532
23:01:58:593, Starting MMTimer... (mmRpTimerId= 16)
23:01:58:593, ftMscLib is initialized ...

23:01:58:593, OpenComDevice(), comStr= COM95
23:01:58:617, ftxOpenComDevice(), ftHandle= 548
23:01:58:618, Starting thread [ReadComThread]...
23:01:58:618, Thread [ReadComThread] started..., hComRead= 552, IdComReadThread= 5608
23:01:58:618, Open Fish.X1 connection...
23:01:58:625, [SetFishX1InfoData] shmId= 0
23:01:58:625,   Hostname          : ROBO TX-509
23:01:58:625,   BtAddress         : 00:13:7B:55:8F:8B
23:01:58:625,   Hardware Release  : C
23:01:58:625,   Firmware Version  : V 1.30
23:01:58:625,   DLL Version       : V 5
23:01:58:625,   SharedMemoryStart : 0x20000204
23:01:58:625,   AppAreaStart      : 0x30700000
23:01:58:625,   AppAreaSize       : 0x000D0000
23:01:58:628, Initialization output and config area...
23:01:58:628, Info Master/Slave alive:  M  0  0  0  0  0  0  0  0
23:01:58:628, InitTransferValues, Initialization of TransferArea (output)...
23:01:58:729, SendRemoteCmd, XM_START: send remote command: 'get_ser_num'
23:01:58:732, SendRemoteCmd, XM_GET_PROMPT: ROBO TX prompt received...
23:01:58:732, serial_number= [0002403770]
23:01:58:732, Starting Fish.X1 transfer...
23:01:58:732, SetFishX1TransferStatus, set status = 2
23:01:59:003, SetFishX1TransferStatus, set status = 1
23:01:59:003, Fish.X1 transfer running...
23:02:09:462, Stopping Fish.X1 transfer...
23:02:09:462, SetFishX1TransferStatus, set status = 0
23:02:09:462, Fish.X1 transfer stopped ...
23:02:09:462, CloseComDevice, ftHandle= 548
23:02:09:462, cancel thread [ReadComThread]...
23:02:09:463, Stopped MmTimer (mmRpTimerId= 16)...
23:02:09:463, Threads terminated...
23:02:09:463, Closing event handles...
23:02:09:463, ftMscLib closed.
