--------------------------------------------------------------------------------
FtMscLib.dll Version  01.05.11  (2012/02/19)
FtLogLevel= 0
22:45:48:217, Initialization of Library 'ftMscLib.dll' ...

INFO:   size FTX1_SHMIFINFO   = 64
INFO:   size FTX1_STATE       = 100
INFO:   size FTX1_CONFIG      = 88
INFO:   size FTX1_INPUT       = 68
INFO:   size FTX1_OUTPUT      = 44
INFO:   size FTX1_DISPLAY     = 108
INFO:   size TRANSFER_STATUS  = 4
INFO:   size CHANGE_STATE     = 8
INFO:   size RP_TIMER         = 12
INFO:   size MOTOR            = 24
INFO:   size INPUT_SIM        = 4
INFO:   size HOOK_TABLE       = 140
INFO:   RESERVE_SIZE          = 360
INFO:   size FISH_X1_TRANSFER = 1024
INFO: size IF08_MAX           = 9
INFO: size IF08_TRANSFER      = 9216

22:45:48:217, Creating event objects...
22:45:48:217, Starting thread [WaitMmRpTmEvent]...
22:45:48:217,   [WaitMmRpTmEvent] started, hRpTmThrWait= 480
22:45:48:217, Starting thread [WaitMmEvent]...
22:45:48:217,   [WaitMmEventThread] started, hThrWait= 488
22:45:48:217, Starting thread [FtRequestThread]...
22:45:48:217,   [FtRequestThread] started, hThrRequest= 492
22:45:48:233, Starting MMTimer... (mmRpTimerId= 16)
22:45:48:233, ftMscLib is initialized ...

22:45:48:233, OpenComDevice(), comStr= COM95
22:45:48:243, ftxOpenComDevice(), ftHandle= 508
22:45:48:243, Starting thread [ReadComThread]...
22:45:48:243, Thread [ReadComThread] started..., hComRead= 512, IdComReadThread= 3888
22:45:48:243, Open Fish.X1 connection...
22:45:48:248, [SetFishX1InfoData] shmId= 0
22:45:48:248,   Hostname          : ROBO TX-509
22:45:48:248,   BtAddress         : 00:13:7B:55:8F:8B
22:45:48:248,   Hardware Release  : C
22:45:48:248,   Firmware Version  : V 1.30
22:45:48:248,   DLL Version       : V 5
22:45:48:248,   SharedMemoryStart : 0x20000204
22:45:48:248,   AppAreaStart      : 0x30700000
22:45:48:248,   AppAreaSize       : 0x000D0000
22:45:48:251, Initialization output and config area...
22:45:48:251, Info Master/Slave alive:  M  0  0  0  0  0  0  0  0
22:45:48:251, InitTransferValues, Initialization of TransferArea (output)...
22:45:48:352, SendRemoteCmd, XM_START: send remote command: 'get_ser_num'
22:45:48:355, SendRemoteCmd, XM_GET_PROMPT: ROBO TX prompt received...
22:45:48:355, serial_number= [0002403770]
22:45:48:355, Starting Fish.X1 transfer...
22:45:48:355, SetFishX1TransferStatus, set status = 2
22:45:48:628, SetFishX1TransferStatus, set status = 1
22:45:48:628, Fish.X1 transfer running...
22:45:56:390, Stopping Fish.X1 transfer...
22:45:56:390, SetFishX1TransferStatus, set status = 0
22:45:56:390, Fish.X1 transfer stopped ...
22:45:56:390, CloseComDevice, ftHandle= 508
22:45:56:390, cancel thread [ReadComThread]...
22:45:56:390, Stopped MmTimer (mmRpTimerId= 16)...
22:45:56:390, Threads terminated...
22:45:56:390, Closing event handles...
22:45:56:390, ftMscLib closed.
